**BATT®-X**

The BATT®-X (Ballistic Armored Tactical Transport®) is the Big Brother to the BATT®-APX. Additional length is added to the APX to allow the BATT®-X to carry 12-14 Officers (depending on size of operators and amount of gear). It is for law enforcement agencies and tactical teams to carry out missions in both rural and urban settings. The Armored Group (TAG) designed the BATT®-X series of vehicles using input provided by tactical teams around the world. The BATT®-X series stems from a need for vehicles that offer protection, comfort, ease of maintenance, storage, and maneuverability superior to the competition.

BATT®-X Features

Our BATT®-X series includes features that add a higher level of comfort and safety than most other armored vehicles. We designed the BATT®-X series to accommodate fully geared officers comfortably and with the utmost security. BATT®-X models include, but are not limited too the following options:

* B7/NIJ IV+ .50 Cal Ball Ammo Protection or B6/NIJ III Armor Levels
* Blast mitigating floor.
* Internal armored firewall.
* Rifle-rated roof protection.
* Fully armored hood clip.
* TAG Exclusive Flip Forward Front Clip System
* Best-in-class climate control system.
* Dual heating and air conditioning systems in front and back.
* Oversized rear deployment bumper with steps.
* Front door lockout ability at 90° and 45°.
* Rear door lockout ability at 90° and at full open
* Heavy Duty Oversized Running Boards
* Optic-ready gun ports.
* Four-wheel drive off-road capabilities.
* Enclosed under-seat storage in rear compartment with back board slat cut outs
* 360° Rotating Turret with Oversized flush-mounted sniper step.
* Roof Hatches
* Emergency Lights and Siren System

We based the BATT®-X on the Ford F-550 4x4 chassis, available in either gas or diesel engines. The diesel version offers more torque and a faster throttle response, while the gas model is quieter and less expensive, but still offers adequate horsepower. The BATT®-X can achieve highway speeds of over 80 miles an hour (128 kph) with 12 to 14 fully geared officers inside.

Why Choose BATT®-X?

The engineers at TAG wanted to give teams a new and innovative APC/rescue vehicle that offered more advantages to complete their missions. The BATT®-X has everything other armored personnel carriers (APCs) on the market lack. BATT-X vehicles come armored in Level NIJ IV/B7+.50 Cal Ball Ammo and NIJ III/B6 Levels. This means they have the highest level of car armor protection, as classified by the National Institute of Justice (NIJ). Level B7 ballistic armor can defend against armor piercing rifle fire and .50 caliber ball ammo rounds. Your team will have the ultimate protection in the BATT®-X.

Specialty and Customizations

All the Ballistic Armored Tactical Transport® (BATT® Vehicles) at The Armored Group, LLC, are customizable. Our design team and engineers will work with you to come up with the perfect BATT®-X vehicle for your needs. You can add our TAG exclusive Multi Angle Hydraulic Ram system, Ram Cameras, Gas Needles, multiple lighting packages, 4 Doors, Off Road Kits, CBRNE package for detection of gases and radiation, LRAD, and many, many more options.

The BATT®-X vehicle you receive from The Armored Group, LLC, is one-of-a-kind, built specifically for your team. We offer patented features that are not available anywhere else, such as our flip-forward hood and multi-angle hydraulic ram system. [Contact us today](http://www.armoredcars.com/contact-us.php) to learn more about the BATT®-X.